Upgrading to GPWS V2.0  when you have V1.0 installed.
=====================================================

Installation
============
- Just install all files as specified in the README 2.0
  There is no need to remove the V1.0 files.
- Overwrite existing files when asked.
  Note that all sounds, sound.ini and the GPWS_sound.gau are unchanged
- All gauge files (.xml and .bmp's) in \Gauges\rcb-gauges\ are now called GPWS2*.
- You need to change the panel.cfg definition of the gauge (GPWS becomes GPWS2).
  Moreover, the gauge size has changed due to the added switches/lights.
  Default size: 82*31 pixels (or any scaled value to suit your panel).


Functionality
=============
See also the README 2.0.

Changes compared to V1.0:
- Each of the 8 modes can now be operated/configured individially, i.e.
  they have there own switch/light.
  A (or more) Modes can even be disabled permanently.
- The seperate testmode has been removed; "test" is now automatically performed
  when the gauge is set from Off to On.
- The "auto-enable" function has been removed. 
  Not needed anymore, since each Mode can now be operated individually.
- The TOGA mode has been visualised by a switch/light. Besides the automatic
  change, it can also be toggle manually.

Enjoy, and fly safe .....

Rob Barendregt, The Netherlands
Email: rc.barendregt@planet.nl


***************************** End Of Readme ********************************

