BAe/SNIAS Concorde
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the aircraft directory. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 404,353 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 530 KIAS >FL320
MMO - Maximum Operating Speed Mach | 2.04 Mach >FL500
VLO - Maximum Gear Operating Speed | 270 KIAS/.7 Mach
VLE - Maximum Landing Gear Extension Speed | 270 KIAS/.7 Mach
VLA - Lowest Authorized Speed (FL150-FL410) | 250KIAS
VLA - Lowest Authorized Speed (FL410-FL600) | 300KIAS

Maximum Nose/Visor Speeds

Nose Position | Speed
Visor Down | 325 KIAS/.8 Mach
5 | 325 KIAS/.8 Mach
12 | 270 < FL200

V1 - Takeoff Decision Speed dry runway
Standard temperature, sea level pressure altitude

Max | 190 KIAS
Min | 120 KIAS

VR - Rotation Speed dry runway
Standard temperature, sea level pressure altitude

Max | 205 KIAS
Min | 139 KIAS

V2 - Takeoff Safety Speed dry runway
Standard temperature, sea level pressure altitude

Max | 225 KIAS
Min | 175 KIAS

VREF - Landing Approach Speed, nose and gear down

Max | 162 KIAS
Min | 150 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.